{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"merged":[[0,0,0,9],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,7],[1,8,2,8],[1,9,2,9],[30,0,30,9]],"flags":["formulas_cached_only"]}
["工程量报价清单"]
["序号","项目名称及特征","单位","工程量   （暂估）","不含税增值税综合单价","合价","甲方供应材料",null,"工程量计算规则","备 注"]
[{"$nulls":6},"材料名称","主材损耗或消耗量"]
[null,"厂内西北侧开槽排水"]
[1,"1、名称：搅拌站原有路面破除\n2、破除厚度：200mm","m3",15.42,null,null,"/","/","按设计图示尺寸以体积计算"]
[2,"1、名称：排水沟沟槽土方开挖\n2、具体详施工图纸","m3",40.06,null,null,"/","/","按设计图示尺寸以体积计算"]
[3,"1、名称：排水沟土方回填\n2、具体详施工图纸","m3",10,null,null,"/","/","按设计图示尺寸以体积计算"]
[4,"1、名称：排水沟土方弃置\n2、具体详施工图纸","m3",32.06,null,null,"/","/","按设计图示尺寸以体积计算"]
[5,"1、名称：搅拌站排水沟垫层\n2、材料名称：C20商砼（非泵送）","m3",7.84,null,null,"混凝土",{"v":0.015,"d":"1.50%"},"按设计图示尺寸以体积计算"]
[6,"1、名称：砖砌排水沟\n2、煤矸石普通砖\n3、墙面1:3水泥砂浆内侧抹灰","m3",5.78,null,null,"/","/","按设计图示尺寸以体积计算"]
[7,"1、名称：搅拌站沉淀池\n2、煤矸石普通砖\n3、墙面1:3水泥砂浆内侧抹灰","m3",0.54,null,null,"/","/","按设计图示尺寸以体积计算"]
[8,"1.名称:雨水篦子\n2.材质、规格:φ22钢筋焊接篦子\n3.规格：450*600","m",107.9,null,null,"/","/","按设计图示尺寸以m计算"]
[9,"1.名称:沉淀池盖板\n2.材质、规格:φ22钢筋焊接沉淀池盖板","m2",1,null,null,"/","/","按设计图示尺寸以㎡计算"]
[null,"2#罐车装料区环保密封棚安装"]
[10,"1、名称：原有损坏围挡拆除\n2、具体详施工现场","m2",70.15,null,null,"/","/","按设计图示尺寸以㎡计算"]
[11,"1、屋面彩钢瓦\n2、0.2mm厚米白色彩钢瓦单板\n3、燕尾螺丝与方管连接\n4、具体详施工图纸","m2",36.58,null,null,"/","/","按设计图示尺寸以㎡计算"]
[12,"1、屋面龙骨\n2、材质规格：40*60*1.5厚冷镀锌方管","t",0.36,null,null,"/","/","按设计图示尺寸以t计算"]
[13,"1、名称：墙面彩钢板\n2、1.5mm厚彩钢瓦\n3、具体详施工图纸","m2",37.25,null,null,"/","/","按设计图示尺寸以㎡计算"]
[14,"1、名称：墙面彩钢板\n2、0.2mm厚彩钢瓦\n3、具体详施工图纸","m2",47.25,null,null,"/","/","按设计图示尺寸以㎡计算"]
[15,"1、名称：墙面龙骨\n2、规格：40*40*1.5\n3、具体详施工图纸","t",0.32,null,null,"/","/","按设计图示尺寸以t计算"]
[16,"1、名称：出料口屋顶支撑\n2、材料：40*40*2镀锌角钢\n3、具体详施工图纸","t",0.02,null,null,"/","/","按设计图示尺寸以t计算"]
[17,"1.柱类型:80*80*1.5mm厚冷镀锌方管\n2.部位:雨棚柱\n3、具体详施工图纸","t",0.3,null,null,"/","/","按设计图示尺寸以t计算"]
[18,"1、名称：出料口柱脚混凝土\n2、材料：C30商砼（非泵送）","m3",0.15,null,null,"混凝土",{"v":0.015,"d":"1.50%"},"按设计图示尺寸以m³计算"]
[19,"1、名称：钢柱预埋钢板\n2、规格：200*200*10\n3、含膨胀螺栓","t",0.02,null,null,"/","/","按设计图示尺寸以t计算"]
[20,"1、用于现场零工，满足8小时","工日",5,null,null,"/","/","以实际确认工日数量为准"]
[21,"1.零工不足4小时，用此清单项计量","小时",8,null,null,"/","/","以实际确认工时数量为准"]
[]
[null,"合计（不含增值税）"]
[null,"增值税（3%）",{"$nulls":3},{"v":0,"d":"0.00"}]
[null,"合计（含增值税）",{"$nulls":3},{"v":0,"d":"0.00"}]
["  以上综合单价包括除增值税外完成招标内容所需的全部费用且综合单价不因工程量发生变化进行调整，包括但不限于人工费、材料设备采购费（甲供材料设备除外）、辅材费、机械机具费、技术服务（包含但不限于施工测量放线等）、措施费（含脚手架）、临时设施费、保险费、停滞费、风雨季及冬季施工费、各种管理费、利润、规费、农民工综合保险、乙方自购材料的涨跌风险及自购材料检验试验费、各种补贴、质量缺陷整改费用，未交付前的半成品及成品保护费、自购材料的采管费、甲供材料的保管费、安全生产费、二次倒运费、安全文明施工费（包含但不限于项目安全生产管理等相关活动）、确保工程施工、质量、进度的一切措施费、临时设施费、窝工费、风雨季及冬季施工费、建筑红线内材料及机械设备搬运费、甲供材料进场卸货、码堆、配合取样送检和施工完后的余料清理、码堆、退库装卸等费用、以及政策性文件规定、合同所有责任、义务和风险费用等。    "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}